19.Τεχνικές προδιαγραφές BARCODE PRINTER

	Α/Α
	ΠΕΡΙΓΡΑΦΗ
	ΑΠΑΙΤΗΣΗ
	ΑΠΑΝΤΗΣΗ
	ΠΑΡΑΠΟΜΠΗ

	1.
	Γενικά
	
	
	

	
	Ποσότητα
	10
	
	

	
	Καινούργιο και αμεταχείριστο
	ΝΑΙ
	
	

	
	Να αναφερθεί ο κατασκευαστής και το μοντέλο
	ΝΑΙ
	
	

	
	Τεχνολογία εκτύπωσης
	Direct Thermal
	
	

	
	Γλώσσες Προγραμματισμού
	ZPL and EPL
	
	

	
	LED status indicator
	ΝΑΙ
	
	

	
	Single button for feed/pause
	ΝΑΙ
	
	

	
	USB connectivity

	ΝΑΙ
	
	

	
	Ethernet connectivity
	ΝΑΙ
	
	

	
	Πρόγραμμα σχεδιασμού ετικετών του ιδίου κατασκευαστή
	NAI
	
	

	
	Διαστάσεις
	274 × 213 × 191 mm
	
	

	
	Ανάλυση
	203 dpi/8 dots per mm
	
	

	
	Μνήμη
	8 MB Flash (expandable）
8 MB SDRAM
	
	

	
	Πλάτος εκτύπωσης
	Τουλάχιστον 104mm
	
	

	
	Ταχύτητα εκτύπωσης
	Τουλάχιστον 150mm το δευτερόλεπτο
	
	

	
	Αισθητήρες χαρτιού
	· Gap sensor
· open cover sensor
· Black label sensor
· Carbon detection sensor
	
	

	
	Firmware
	ZPL II; EPL 2; DPL
	
	

	
	Μέγιστο μήκος ετικέτας 
	1778 mm
	
	

	
	1D Bar Codes
	Code 11, Code 39, Code 93, Code 128, ISBT-128, 
UPC-A, UPC-E, EAN-8, EAN-13, UPC and EAN 2-or 
5-digit extensions, Plessey, Postnet, Standard 2-of-
5, Industrial 2-of-5, Interleaved 2-of-5, Logmars, 
MSI, Codabar and Planet Code
	
	

	
	2D Bar Codes
	QR, PDF417, Micro PDF417, DataMatrix, Aztec supported
	
	

	
	Fonts and Graphics
	16 ZPL bitmap, 2 scalable, 5 EPL fonts
Unicode compliant for multi-language, on demand 
thermal printing
8 MB user available non-volatile memory, 
8 MB user available SDRAM
	
	

	
	Regulatory
	CE, CCC, RoHS, REACH
	
	

	
	Εγγύηση διάρκειας 1 έτους 
	NAI
	
	







